|  |
| --- |
|  |
| Lower Limbs Table SRS |
| 003 666  **DRAFT 1** |



|  |  |  |  |
| --- | --- | --- | --- |
| Rev | Date | Author | Modifications |
| Draft 1 for v1 | April 4th 2017 | R Heitz | Initial version |
| Draft 2 for v1 | April 10th 2017 | R Heitz | Doc review log corrections |

Contents

[1 Overview 5](#_Toc518565761)

# Overview

This document is the specification of the lower limbs table.

1. The table shall be able to hold people < 150kg
2. The table shall be able to hold people between 70cm and 2m max
3. The table shall allow to dock the stretcher for patient transfer
4. The table shall be in medical sterilisable plastic FDA standard
5. The table shall allow to hold a scanner from 130 to 180 cm height
6. The table shall allow to move the scanner between 1 cm/sec to 10 cm/sec
7. The table shall provide a joystick for motion control
8. The table shall be completely transparent to X-rays
9. The table shall provide restrainers at the ankle and the wraist
10. The table shall comply with the FDA-#1123 regulation